Set the cable on the bracket (A).Turn the adjusting nut (B) so that its free play is 0 mm. Position the adjusting nut on the other side of the bracket, then tighten the locknut (C). K24A3 engine: With the cable properly adjusted, check the throttle link to be sure it opens fully when you push the accelerator pedal to the floor. Also check the throttle link to be sure it returns whenever you release the accelerator pedal. K20A6 engine: With the cable properly adjusted, check the throttle valve to be sure it opens fully when you push the accelerator pedal to the floor. Also check the throttle valve to be sure it returns to the idle position whenever you release the accelerator pedal. |