For K24A3 Engine model 2nd Clutch: Install the waved spring (A) in the clutch drum (B). Install the 4.0 mm-thick plate (C) with the sheer droop side (D) toward the inside of the drum, clutch disc (E), and 2.0 mm-thick flat-plate (F), then starting with the disc, alternately install the discs (G) (4) and waved-plates (H) (3), then install the clutch-end-plate (I) with the flat side toward the disc. |