Yaw Rate/Lateral Acceleration Sensor Replacement

NOTE: Do not damage or drop the sensor as it is sensitive. LHD type: Remove the driver's seat. RHD type: Remove the passenger's seat. Turn up the floor carpet (A). Remove the bracket mounting bolts (B). Remove the yaw rate/lateral acceleration sensor (C) with the bracket (D). Remove the bracket (E). Install in the reverse order of removal. Do the VSA sensor neutral position memorization. |