DTC Troubleshooting: P1095 (95-9)

DTC P1095: Fuel Rail Pressure Control Valve Malfunction Before attempting troubleshooting. Check whether DTC could have been caused by insufficient fuel level. Was fuel insufficient?
YES | - | Supply fuel, and do the fuel system air bleeding, then go to Step 12 .
NO | - | Go to Step 2 .
Note this freeze data: Engine speed Vehicle speed ECT Check the ECT in the freeze data. Could fuel have frozen due to extremely low temperature?
YES | - | Check and repair the freezing point in the low pressure fuel line, then go to Step 12 .
NO | - | Go to Step 4 .
Turn the ignition switch OFF. Check for fuel leaks in the high pressure fuel line (at the injector, fuel pipe, etc.). Is there any leak?
YES | - | Repair the fuel leak in the high pressure fuel line, then go to Step 12 .
NO | - | Go to Step 6 .
Disconnect the low pressure fuel feed hose from the fuel supply pump, and receive fuel in a container. Squeeze the fuel hand primer and operate it 30 times. Does fuel flow out?
YES | - | Go to Step 8 .
NO | - | Replace the fuel filter, then go to Step 12 .
Clear the DTC with the HDS. Do the FUEL RAIL PRESSURE TEST in the INSPECTION MENU with the HDS. Is the result OK?
YES | - | Intermittent failure, system is OK at this time.■
NO | - | Go to Step 10 .
Turn the ignition switch OFF. Replace the fuel supply pump assembly. Turn the ignition switch ON (II). Reset the ECM with the HDS. Start the engine. Check for Temporary DTCs or DTCs with the HDS. Is DTC P1095 indicated?
YES | - | If DTC P1095 is indicated, check for poor connections or loose terminals at the fuel rail pressure sensor, fuel rail pressure control valve and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Troubleshooting is complete.■