Disconnect the negative cable from the battery. NOTE: If you remove the tailgate latch with the battery negative cable still in plugged, the vehicle falls into the fail-safe mode. Remove the tailgate lower trim panel. Disconnect the tailgate latch connector (A). Remove the bolts (B, C), and pull the tailgate latch (D) out, then remove it. Install the latch in the reverse order of removal, and note these items: Make sure the connector is plugged in properly. Reconnect the negative cable to the battery. Reset the clock. Perform the power window control unit reset procedure. Make sure the tailgate opens properly and locks securely. |