1. Remove the center console (A).
   -1. | Open the console box lid (B) then remove the console mat (C).
   -2. | '05 model: Disconnect the rear accessory power socket connector (D), and detach the clip (E).
   -3. | Remove the screws (F, G), then pull up the rear portion of the console up to release the hooks (H), then remove the console.
Install the console in the reverse order of removal, and replace any damaged clips |