DTC P0365: CMP Sensor B No Signal Turn the ignition switch ON (II). Clear the DTC with the HDS. Start the engine. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Is DTC P0365 indicated?
YES | - | Go to Step 5 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at CMP sensor B and the ECM/PCM.■
Turn the ignition switch OFF. Disconnect CMP sensor B 3P connector. Turn the ignition switch ON (II). Measure voltage between CMP sensor B 3P connector terminal No. 3 and body ground. Is there battery voltage?
YES | - | Go to Step 9 .
NO | - | Repair open in the wire between CMP sensor B and PGM-FI main relay 1 (FI MAIN), then go to Step 19 .