Check for continuity between ECM/PCM connector terminal E9 and body ground. Is there continuity?
YES | - | Repair short in the wire between the No. 19 FUEL PUMP (15 A) fuse and the ECM/PCM (E9), or between the No. 19 FUEL PUMP (15 A) fuse and PGM-FI main relay 2 (FUEL PUMP), or between the No. 19 FUEL PUMP (15 A) fuse and the immobilizer control unit. Also replace the No. 19 FUEL PUMP (15 A) fuse.■
NO | - | Go to Step 38 .
Remove the trunk floor trim panel. Remove the access panel from the floor. Disconnect the fuel pump 5P connector. |