Check for continuity between the No. 17 terminal of power tailgate control unit connector A (26P) and body ground. Is there continuity?
YES | - | Go to Step 15 .
NO | - | Go to Step 10 .
By using the screwdriver, close the latch in the tailgate. Connect battery positive (+) terminal to the No. 26 terminal of power tailgate control unit connector A (26P), and connect negative (−) terminal to No. 13 terminal of one. Then, move the motor to closing direction less than one second. |