Apply Molykote M77 grease to the areas indicated by the arrows. Wipe excess grease off the pads (A). Contaminated brake discs or pads reduce stopping ability. Keep grease off the brake discs and pads. Push in the piston (B) so that the caliper will fit over the pads. Install the inner pad to the caliper body, and install the outer pad to the caliper bracket (C). If you are reusing the pads, always reinstall the brake pads in their original positions to prevent a momentary loss of braking efficiency. Install the caliper (D) into position. Install the pin bolts, and torque it to the specified torque being careful not to damage the guide. Install the brake hose mounting bolt, and tighten it to the specified torque. | Inner pad Outer pad