Exploded View Removal Raise the rear of the vehicle, and support it with safety stands in the proper locations. Remove the rear wheel. Place a floor jack under the lower arm B to support the suspension. Remove the lid on the rear side trim panel. Hold the damper shaft (A) with a hex wrench (B), and loosen the self-locking nut (C). Remove the self-locking nut, damper mounting washer (D), and damper mounting rubber (E) from the top of damper. |