Installation Before installing the steering gearbox, make sure that no fluid or grease is on the mating surface of the gearbox and a front suspension subframe. To prevent the gearbox mounting bolts from loosening after the installation, remove the fluid or grease from the mount cushions and bolt holes. Apply a mild soap and water solution to both sides of the mount cushion mating surfaces (A). Pass the motor of the steering gearbox (B) through the wheelwell opening on the driver's side. |