Special Tools Required Handle driver 07749-0010000 Oil seal driver attachment 106 070AD-RCA0200 Check the connecting rod bearing clearance with plastigage. Check the main bearing clearance with plastigage. Install the bearing halves in the engine block and connecting rods. Apply a coat of new engine oil to the main bearings and rod bearings. Install the crankshaft position (CKP) pulse plate (A) to the crankshaft (B). Hold the crankshaft so rod journal No. 2 and rod journal No. 3 are straight up, and lower the crankshaft into the block. |