Start the engine, and then check the showing ‘‘WATER IN/FUEL FILTER'' in the odometer/outside temperature display (A). If the ‘‘WATER IN/FUEL FILTER'' in the odometer/outside temperature display is showing, go to Step 6 . If the ‘‘WATER IN/FUEL FILTER'' in the odometer/outside temperature display is not showing, fuel filter water bleeding is complete. Disconnect the fuel filter water level switch 2P connector, and then recheck the showing ‘‘WATER IN/FUEL FILTER'' in the odometer/outside temperature display. If the ‘‘WATER IN/FUEL FILTER'' in the odometer/outside temperature display is showing, repair short in the wire between the fuel filter water level switch and the gauge assembly. If the ‘‘WATER IN/FUEL FILTER'' in the odometer/outside temperature display is not showing, replace the fuel filter water level switch. Bleed the fuel system. |