Engine Oil Replacement

1. Warm up the engine. Remove the maintenance lid (A). Remove the drain bolt (B), and drain the engine oil. Reinstall the drain bolt with a new washer (C). Refill with the recommended oil. Clean up any spilled engine oil. Run the engine for more than 3 minutes, then check for oil leakage.
   Capacity
   At Oil Change:
   5.5 L (5.8 US qt, 4.8 Imp qt)
   At Oil Change including Filter:
   5.9 L (6.2 US qt, 5.2 Imp qt)
   After Engine Overhaul
   6.5 L (6.9 US qt, 5.7 Imp qt)