1. Lower the roof console (A).
   -1. | Remove the lens (B).
   -2. | With U/S intrusion sensor: Pry up on the front edge of the roof console trim (C) with a flat-tip screwdriver wrapped with protective tape to release the hooks (D), then remove the cover.
   -3. | Remove the bolts (E), then pull out the front individual map light (F).
   -4. | Remove the bolts (G), and if equipped, disconnect the ultrasonic sensor connector (H).
| Without ultrasonic sensor With ultrasonic sensor