DTC Troubleshooting: 27

DTC 27: Steering Angle Sensor Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle around a number of corners. Verify the DTC. Is DTC 64 indicated?
YES | - | Do the appropriate troubleshooting for the DTC.■
NO | - | Go to Step 6 .
Turn the ignition switch OFF. Disconnect the VSA control unit 47P connector, and steering angle sensor 5P connector. Turn the ignition switch ON (II). Measure the voltage between body ground and the VSA control unit 47P connector terminal No. 5, and No. 7 individually. Is there 1 V or more?
YES | - | Repair short to power in the wire between the VSA modulator-control unit and the steering angle sensor.■
NO | - | Go to Step 10 .

Measure the voltage between body ground and the VSA control unit 47P connector terminal No. 3, No. 28, and No. 30 individually. Is there 1 V or more?
YES | - | Repair short to power in the wire between the VSA modulator-control unit and the steering angle sensor.■
NO | - | Go to Step 11 .
Turn the ignition switch OFF. |

Check for continuity between body ground and the VSA control unit 47P connector terminal No. 5, and No. 7 individually. Is there continuity?
YES | - | Repair short to body ground in the wire between the VSA modulator-control unit and the steering angle sensor.■
NO | - | Go to Step 13 .

Check for continuity between body ground and the VSA control unit 47P connector terminal No. 3, No. 28, and No.30 individually. Is there continuity?
YES | - | Repair short to body ground in the wire between the VSA modulator-control unit and the steering angle sensor.■
NO | - | Go to Step 14 .

Check for continuity between the VSA control unit 47P connector terminal No. 5, No. 7 and steering angle sensor 5P connector terminal No. 1, No. 5 individually. Is there continuity?
YES | - | Go to Step 15 .
NO | - | Repair open in the wire between the VSA modulator-control unit and the steering angle sensor.■

Check for continuity between the VSA control unit 47P connector terminal No. 3, No. 28, No. 30 and steering angle sensor 5P connector terminal No. 2, No. 3, and No. 4 individually. Is there continuity?
YES | - | Go to Step 16 .
NO | - | Repair open in the wire between the VSA modulator-control unit and the steering angle sensor.■
Substitute a known-good steering angle sensor. Reconnect all of the disconnected connectors. Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle around a number of corners. Verify the DTC. Is DTC 27 indicated?
YES | - | Replace the VSA modulator-control unit. ■
NO | - | Replace the steering angle sensor. ■