Remove the upper radiator hose (A) and heater hoses (B). Remove the engine wire harness connectors and wire harness clamps from the cylinder head. Four injector connectors Engine coolant temperature (ECT) sensor connector Camshaft position (CMP) sensor A/B connectors K20A6 engine: Exhaust gas recirculation (EGR) valve connector VTEC solenoid valve connector Engine oil pressure (EOP) sensor connector |