Reconnect the cable reel 5P (13P) connector (A) to the dashboard wire harness. ( ): With cruise control Remove the driver's airbag assembly, and disconnect the horn switch 1P positive terminal from the cable reel (B). Using a jumper wire, connect the cable reel side 1P connector (C) to body ground. If the horns sound, replace the driver's airbag assembly. If the horns don't sound, replace the cable reel. |