Engine Mount Positioning

Remove the air cleaner housing. Remove the ground cable (A), then remove the upper torque rod (B). |

Loosen the side engine mount bracket bolt (A). Loosen the side engine mount bracket bolts/nut (B). |

Loosen the transmission upper mount bracket bolt (A). Loosen the transmission upper mount bolt/nuts (B). Raise the vehicle on the hoist to full height. |

Loosen the lower torque rod bolt (A). Lower the vehicle on the hoist. |

Tighten the side engine mount mounting bolts/nut in the numbered sequence shown. |

Tighten the transmission upper mount/bracket mounting bolts/nuts in the numbered sequence shown. Raise the vehicle on the hoist to full height. |

Tighten the lower torque rod mounting bolt. Lower the vehicle on the hoist. |

Install the upper torque rod (A), then tighten the new bolts in the numbered sequence shown. Install the ground cable (B). Install the air cleaner housing. |