Check for continuity between the adaptive cruise control (ACC) unit 20P connector No. 5 terminal and body ground. Is there continuity?
YES | - | Go to Step 20 .
NO | - | Repair an open in the wire between the adaptive cruise control (ACC) unit and the left front pressure sensor.■
Remove the jumper wire from the left front pressure sensor. Reconnect all connectors. Turn the ignition switch ON (II). |