Special Tools Required Ball joint remover, 28 mm 07MAC-SL00201 or 07MAC-SL00200 Removal Note these items during removal: Using solvent and a brush (avoid any electrical part), wash any oil and dirt off the end of the gearbox. Blow dry with compressed air. Make sure to remove the steering wheel before disconnecting the steering joint. Damage to the cable reel can occur. Make sure you have the anti-theft codes for the radio, then write down the customer's radio station presets. Remove the battery. Raise the front of vehicle, and support it with safety stands in the proper location. Remove the front wheels. Remove the steering wheel. Remove the steering joint cover A. |