1. Install the cylinder head in the reverse order of removal. Clean the cylinder head, piston head, and block surface. Inspect the cylinder head warpage. Measure the piston head projection value for each cylinder using the dial indicator.
   -1. | Set the dial indicator (A) on the block.
   -2. | Zero the dial indicator at the point B on the block, then measure the projection value at the point C on the piston head. Do the same procedure at the point D, after zero the indicator at the point E.
   -3. | Average of the measured values.
   -4. | Measure the piston head projection value at other three pistons, and note the highest piston head projection value.