DTC Troubleshooting: 66

DTC 66: VSA Pressure Sensor (Inside of VSA Modulator-Control Unit) Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle. Does the ABS indicator come on, and is DTC 66 indicated?
YES | - | Go to Step 5 .
NO | - | The system is OK at this time.■
Do the VSA sensor neutral position memorization. Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle. Does the ABS indicator come on, and is DTC 66 indicated?
YES | - | Replace the VSA modulator-control unit. ■
NO | - | The system is OK at this time.■