Oil pump

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Oil pump | Inner-to-outer rotor clearance |  | 0.02−0.14 mm (0.0008−0.0055 in.) | 0.19 mm (0.0075 in.)
Pump housing-to-outer rotor clearance |  | 0.15−0.21 mm (0.006−0.008 in.) | 0.23 mm (0.009 in.)
Pump housing-to-rotor axial clearance |  | 0.020−0.055 mm (0.0008−0.0022 in.) | 0.10 mm (0.004 in.)