Maintenance Schedule for Normal Conditions
100,000km(5year)

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first

| Replace engine oil

| Replace engine oil filter

| Drain fuel filter

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad, front disc, rear pad, rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

| Check lights alignment
Check the position of the headlights

| Test drive (noise, stability, dashboard operation)

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease

| Brake hoses and lines (including VSA)
Check the master cylinder, proportioning control valve, and VSA modulator-control unit and leakage

| All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, and engine coolant, MTF , brake fluid, power steering fluid, and windshield fluid

| Exhaust system
Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness

| Fuel lines and connections
Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

| Tyre condition

Every 40,000 km (25,000 miles)

| Replace air cleaner element

At 100,000 km (62,500 miles) or 5 years, then every 60,000 km (37,500 miles) or 3 years

| Replace engine coolant
Use genuine Honda Long Life Antifreeze/ Coolant Type 2

Every 120,000 km (75,000 miles) or 8 years

| Replace manual transmission fluid
Use genuine Honda MTF

Every 3 years

| Replace brake fluid
|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level between the upper and lower marks on the reservoir

Every year

| Inspect vehicle corrosion
Paintwork and bodywork check