NOTE: Use fender covers to avoid damaging painted surfaces. Write down the frequencies for the radio's preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery. Remove the air cleaner housing. Remove the battery base. Carefully remove the slave cylinder so as not to bend the clutch line. Do not operate the clutch pedal once the slave cylinder has been removed. |