Apply multipurpose grease to the sliding surfaces of the regulator (A) where shown. Install the glass and regulator in the reverse order of removal, and note these items: Never use any kind other than the corrosion-resistant bolts where these special bolts are originally installed. If other bolts are used, electrolysis may accelerate corrosion around tightening points, resulting in loosening of the joints. Roll the glass up and down to see if it moves freely without binding. Make sure that there is no clearance between the glass and glass run channel when the glass is closed. Adjust the position of the glass as necessary. Check for water leaks. Test-drive and check for wind noise and rattles. When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its perimeter. |