Maintenance Schedule for Normal and Severe Conditions - Except EU

This Maintenance Schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of the vehicle. Due to regional and climatic differences, some additional service may be required. Please consult the warranty booklet for a more detalied description.
The following items must be used for ‘‘severe conditions'' indicated on schedule, if the vehicle is driven MAINLY under the specified conditions A to E.

- Engine oil and engine oil filter: A/B/C/D/E
- Air cleaner element: D/E
- Transmission fluid: B/D

A: Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
B: Driving in extremely hot over 35 °C (95 °F) conditions.
C: Extensive idling, or long periods of stop-and-go driving.
D: Trailer towing, driving with a loaded roof rack, or driving in mountainous conditions.
E: Driving on muddy, dusty, or de-iced roads.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil and filter | Normal conditions | Every 10,000 km (6,250 miles) or 1 year
Severe conditions | Every 5,000 km (3,125 miles) or 6 months
Replace air cleaner element | Normal conditions | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Severe conditions | Every 10,000 km (6,250 miles)
Replace fuel filter Replace fuel filter every 40,000 km (25,000 miles) or 2 years, if the fuel the customer uses is suspected to be contaminated. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Inspect drive belt Look for cracks and damage, then check the position of the drive belt auto-tensioner indicator. |  | ● |  | ● |  | ● |  | ● |  | ●
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2. |  |  |  |  | ● |  |  | ● |  |
Replace Manual Transmission Fluid (MTF) Use genuine Honda MTF. | Normal Conditions |  |  |  |  |  | ● |  |  |  |
Severe Conditions |  |  | ● |  |  | ● |  |  | ● |

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Check front and rear brakes Check the brake pad and disc thickness. Check for damage or cracks. | Every 10,000 km (6,250 miles) or 6 months
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid. Check the brake fluid level is between the upper and lower marks on the reservoir. | Every 3 years
Check parking brake adjustment Check the parking brake operation. | ● | ● |  | ● |  | ● |  | ● |  | ●
Replace dust and pollen filter | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Rotate tyres Check tyre inflation at least once per month. | Every 10,000 km (6,250 miles)
Visually inspect the following items: Check for correct installation and position, check for cracks, deterioration, rust, and leaks. Check tightness of screws, nuts, and joints. If necessary, retighten.
Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease. | Every 10,000 km (6,250 miles) or 6 months
Suspension components Check the bolts for tightness. Check all dust covers for deterioration and damage.
Driveshaft boots Check the boot and boot band for cracks. Check rack grease.
Brake hoses and lines (including VSA lines) Check the master cylinder and VSA modulator-control unit and leakage. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
All fluid levels and condition of fluid Check levels and check for leaks. If necessary, add. Engine coolant MTF Clutch fluid Power steering fluid Brake fluid Windshield fluid
Exhaust system Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness.
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts.