How to display DTC on the gauge control module While in mode 1, the DTCs which have been detected and stored individually by various B-CAN (Body-controller Area Network) units, will be shown one by one on the ODO display when the communication between the MICU (Multiplex Integrated Control Unit) and the gauge control module is normal. To scroll through the DTCs, press the reset switch on the gauge control module.