1. To remove a rear drain valve (A) from the body, remove these parts: Spare tyre lid
   - | Without trunk side spacer
   - | With trunk side spacer
   Trunk side spacer, if equipped Trunk rear trim panel
   - | Without trunk side spacer
   - | With trunk side spacer
Tie a string to the top end of the rear drain tube (B), then pull back the trunk side trim panel and pull the drain tube down out of the pillar leaving the string inside the pillar. |