DTC Troubleshooting: 32-1x, 32-2x

DTC 32-1x (32-10 to 32-19, 32-1A to 32-1F): Open in Right Side Airbag Inflator DTC 32-2x (32-20 to 32-29, 32-2A to 32-2F): Increased Resistance in Right Side Airbag Inflator Special Tools Required SRS inflator simulator 07SAZ-TB4011A SRS simulator lead E 07XAZ-S1A0200 Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 32-1x or 32-2x indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. Disconnect the floor wire harness 2P connector (A) from the right side airbag. Connect the SRS inflator simulator (2 Ω connector) and simulator lead E to the floor wire harness. Reconnect the battery negative cable. Erase the DTC memory. Read the DTC. Is DTC 32-1x or 32-2x indicated?
YES | - | Go to Step 9 .
NO | - | Open or increased resistance in the right side airbag inflator, replace the right side airbag. ■
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. |

Disconnect both seat belt tensioner 4P connectors (A). |

Disconnect SRS unit connector B (28P) from the SRS unit. Do not disconnect the simulator lead from floor wire harness. Disconnect the SRS inflator simulator from the SRS simulator lead. |

Check resistance between the terminals of SRS simulator lead. There should be 1.0 Ω or less. Is the resistance as specified?
YES | - | Faulty SRS unit or poor contact at SRS unit connector B (28P) and the SRS unit. Check the connection; if the connection is OK, replace the SRS unit. ■
NO | - | Open or increased resistance in the floor wire harness; replace the floor wire harness.■