Install in the reverse order of removal. Make sure the crimped side of the ring terminal is facing out. Connect the positive cable to the battery first, then connect the negative cable. Start the engine to make sure the starter works properly. Enter the anti-theft codes for the radio and the navigation system, then enter the customer's radio station presets. Set the clock. Do the power window control unit reset procedure. |