Press the brake pedal. Are the brake lights ON?
YES | - | Go to Step 2 .
NO | - | Repair faulty brake light circuit.■
Connect the HDS. Check engine speed and throttle position in the A/T data list. Is the engine speed at idle, and TPS about 0.5 V?
YES | - | Go to Step 3 .
NO | - | Repair engine speed or throttle position input.■
Choose Shift Lock Solenoid Test in Miscellaneous Test Menu, and check that the shift lock solenoid operates with the HDS. Does the shift lock solenoid work properly?
YES | - | Shift lock system is OK. Check the shift lock mechanism if necessary.■
NO | - | Go to Step 4 .
Turn the ignition switch OFF. Remove the center console. Disconnect the shift lock solenoid connector. Turn the ignition switch ON (II). Measure the voltage between No. 1 terminal of the shift lock solenoid connector and body ground. Is there battery voltage?
YES | - | Go to Step 7 .
NO | - | Check for blown No. 21 fuse in the under-dash fuse/relay box. If the fuse is OK, repair open in the wire between the shift lock solenoid connector and the under-dash fuse/relay box.■
Shift the shift lever into the P position, and press the brake pedal. |