Check for continuity between radiator fan motor 2P connector terminal No. 1 and body ground. Is there continuity?
YES | - | Replace the radiator fan motor.■
NO | - | Check for an open in the wire between radiator fan motor 2P connector terminal No. 1 and body ground. If the wire is OK, check for a poor ground at G301.■
Reinstall the radiator fan relay. Disconnect the radiator fan switch 2P connector. |