Remove the hub bearing unit (A). Install the hub bearing unit in the reverse order of removal, and note these items: Tighten all mounting hardware to the specified torque values. Use a new spindle nut on reassembly. Wash the spline thoroughly in high flash point solvent before reassembly. Before installing the spindle nut, apply a small amount of engine oil to the seating surface of the nut. After tightening, use a drift to stake the spindle nut shoulder against the driveshaft. Before installing the brake disc/drum, clean the mating surfaces of the hub bearing unit and the brake disc/drum. Before installing the wheel, clean the mating surfaces of the brake disc/drum and the inside of the wheel. Check the wheel alignment, and adjust it if necessary. |