Steering-related Precautions Cable Reel Alignment Misalignment of the cable reel could cause an open in the wiring, making the SRS system and the horns inoperative. Center the cable reel whenever the following is performed.
- | Installation of the steering wheel
- | Installation of the cable reel
- | Installation of the steering column
- | Other steering-related adjustment or installation
Do not disassemble the cable reel. Do not apply grease to the cable reel. If the cable reel shows any signs of damage, replace it with a new one. For example, if it does not rotate smoothly, replace the cable reel. |