Cautions for the Vehicle All wheels of the vehicle should touch the ground. Make sure that the suspensions are not modified. Check the air pressure of all the tyres. If the pressures are uneven, inflate the tyres to the specified value. Do not place the wheels of the vehicle on a steel plate or a roller when performing the aiming. The vehicle should be empty and not be loaded when performing the aiming. NOTE: Empty vehicle: A full fuel tank, tools and a spare tyre are present. Unload any baggage other than and the spare tyre. Make sure that all doors are closed when performing the aiming. Do not put any objects on the instrument panel. Make sure that there are no stains on the lens of the LKAS camera, and the interior and exterior surface of the front glass of the lens parts. Set the steering wheel in the straight ahead position. Do not operate the steering wheel after the vehicle is set in the aiming position. Shift the lever to the P position and apply the parking brake. If you are towing a trailer, unhitch the trailer. |