DTC 22-1x (22-10 to 22-19, 22-1A to 22-1F): Open in Right Side Seat Belt Tensioner DTC 22-2x (22-20 to 22-29, 22-2A to 22-2F): Increased Resistance in Right Side Seat Belt Tensioner Special Tools Required SRS inflator simulator 07SAZ-TB4011A SRS simulator lead F 07XAZ-SZ30100 Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 22-1x or 22-2x indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. Disconnect the right side seat belt tensioner 4P connector (A) from the floor wire harness. Connect the SRS inflator simulator (2 Ω connectors) and simulator lead F to the floor wire harness. Reconnect the battery negative cable. Erase the DTC memory. Read the DTC. Is DTC 22-1x or 22-2x indicated?
YES | - | Go to Step 9 .
NO | - | Open or increased resistance in the right side seat belt tensioner; replace the Right side seat belt. ■
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. |