DTC 51: Motor Lock DTC 52: Motor Stuck OFF Check the No. 17 (30 A) fuse in the under-hood fuse/relay box. Is the fuse OK?
YES | - | Reinstall the fuse, and go to Step 2 .
NO | - | Replace the fuse, and recheck.■
Disconnect the VSA control unit 47P connector. Measure the voltage between the VSA control unit 47P connector terminal No. 1 and body ground. Is there battery voltage?
YES | - | Go to Step 4 .
NO | - | Repair open in the wire between the No. 17 (30 A) fuse and the VSA modulator-control unit.■