DTC P1731: Problem in Shift Control System: Shift Solenoid Valve E Stuck ON Shift Valve E Stuck A/T Clutch Pressure Control Solenoid Valve A Stuck OFF NOTE: Record all freeze data and review General Troubleshooting Information before you troubleshoot. Warm up the engine to normal operating temperature (the radiator fan comes on). Make sure that the transmission is filled to the proper level, and check for fluid leaks. Drain the ATF through a strainer. Inspect the strainer for metal debris or excessive clutch material. Does the strainer contain metal debris or excessive clutch material?
YES | - | Replace the transmission.■
NO | - | Replace the ATF, then go to Step 4 .
Clear the DTC with the HDS. Test-drive the vehicle in the D position in all five gears at speeds over 20 km/h (12 mph) for more than 20 seconds, then slow down to a stop. Retest-drive the vehicle in the D position in all five gears at speeds over 20 km/h (12 mph) for more than 20 seconds, then slow down to a stop. Monitor the OBD status for P1731 in the DTCs/Freeze Data in A/T Mode Menu for a pass/fail. Does the result indicate a fail?
YES | - | Go to Step 8 .
NO | - | Intermittent failure, the system is OK at this time. If the tester indicates NOT COMPLETE, return to Step 5 and recheck.■
Clear the DTC with the HDS. Choose Shift Solenoid E in Miscellaneous Test Menu, and check that the shift solenoid valve E operates with the HDS. Is a clicking sound heard?
YES | - | Go to Step 10 .
NO | - | Replace shift solenoid valve E, then go to Step 12 .
Choose Clutch Pressure Control (Linear) Solenoid A in Miscellaneous Test Menu, and test the A/T clutch pressure control solenoid valve A with the HDS. Is the system OK?
YES | - | Intermittent failure, the system is OK at this time. If the tester indicates NOT COMPLETE, return to Step 10 and recheck.■
NO | - | Follow instructions indicated on the HDS by the test result, but the tester has not determined the cause of the failure, go to Step 11 . If any part is replaced, go to Step 12 .
Inspect A/T clutch pressure control solenoid valve A. Does the A/T clutch pressure control solenoid valve A work properly?
YES | - | Repair hydraulic system related with shift valve E, or replace the transmission, then go to Step 12 .
NO | - | Replace A/T clutch pressure control solenoid valve A, then go to Step 12 .
Clear the DTC with the HDS. Test-drive the vehicle in the D position in all five gears at speeds over 20 km/h (12 mph) for more than 20 seconds, then slow down to a stop. Retest-drive the vehicle in the D position in all five gears at speeds over 20 km/h (12 mph) for more than 20 seconds, then slow down to a stop. Monitor the OBD status for P1731 in the DTCs/Freeze Data in A/T Mode Menu for a pass/fail. Does the result indicate a pass?
YES | - | The problem has been corrected.■
NO | - | Return to Step 8 and recheck.■