Install the servo body (11 bolts). Install the ATF strainer with the two bolts in the bolt holes (A) in step 12, and install the baffle plate with the two bolts in the bolt holes (B) in step 2 in shaft assemblies and housing installation. Install the regulator separator plate and two dowel pins on the main valve body. Install the new O-ring on the stator shaft, and install the stator shaft and stator shaft stop. Install the regulator valve body (eight bolts). Install the new O-ring on the ATF strainer, and install the ATF strainer (two bolts). Install the ATF joint pipes (one bolt). Install the ATF feed pipes in the regulator valve body and servo body. |