With a helper on the outside, pull the piano wire (A) back and forth in a sawing motion. Hold the piano wire as close to the quarter glass (B) as possible to prevent damage to the body, and carefully cut through the adhesive (C) around the entire quarter glass: If the quarter glass is to be reinstalled, take care not to damage the molding (D). If the molding is damaged, replace the quarter glass, molding, and clips (E) as an assembly. If any of the clips are broken, the quarter glass can be reinstalled using butyl tape (refer to Step 10 ). Carefully remove the quarter glass. With a putty knife, scrape the old adhesive smooth to a thickness of about 2 mm (0.08 in.) on the bonding surface around the entire quarter glass opening flange: Do not scrape down to the painted surface of the body; damaged paint will interfere with proper bonding. Remove the clips and fastener from the body. Clean the body bonding surface with a sponge damaged in alcohol. After cleaning, keep oil, grease, and water from getting on the surface. | Cutting positions