At solenoid side, measure resistance between IMRC solenoid valve 2P connector terminals No. 1 and No. 2. Is there about 33 Ω at room temperature?
YES | - | Go to Step 16 .
NO | - | Go to Step 10 .
Replace the IMRC solenoid valve. Reconnect all connectors. Turn the ignition switch ON (II). Reset the ECM with the HDS. Start the engine. Hold the engine speed at 2,000 rpm (min −1 ) without load (in neutral) until the radiator fan comes on, then let it idle. Check for Temporary DTCs or DTCs with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P2009 is indicated, check for poor connections or loose terminals at the IMRC solenoid valve and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Troubleshooting is complete.■
Update the ECM if it does not have the latest software, or substitute a known-good ECM. Start the engine. Hold the engine speed at 2,000 rpm (min −1 ) without load (in neutral) until the radiator fan comes on, then let it idle. Check for Temporary DTCs or DTCs with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P2009 is indicated, check for poor connections or loose terminals at the IMRC solenoid valve and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | If the ECM was updated, troubleshooting is complete. If the ECM was substituted, replace the original ECM. ■