A/T Housing Reverse Idler Gear Removal and Installation

Removal Remove the bolt (A) securing the reverse idler gear shaft holder. Install a 5 x 0.8 mm bolt (B) in the reverse idler gear shaft, and pull it to remove the reverse idler gear shaft (C) and gear shaft holder (D) together. |

Remove the reverse idler gear. |

Installation Install the reverse idler gear in the transmission housing. Lightly coat the reverse idler gear shaft (A), needle bearing (B), and new O-rings (C) with lithium grease. Assemble the new O-rings and needle bearing on the reverse idler gear shaft, then install the reverse idler gear shaft in the reverse idler gear shaft holder (D). Align the D-shaped cut out (E) of the shaft with the D-shaped area (F) of the holder. |

Install the reverse idler gear shaft/holder assembly on the transmission housing. |