Write down the frequencies for the radio's preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery. Remove the air cleaner housing. Remove the battery base. Carefully remove the shift cable, select cable, and cable bracket together so as not to bend the cables. Disconnect the mainshaft speed sensor connector, back-up light switch connector, and reverse lockout solenoid connector. Remove the bolts (A) and reverse lockout solenoid (B). |