Exploded View NOTE: Refer to the exploded view as needed during the following procedures. Make sure that the ATF magnet is cleaned and installed in the torque converter housing. Install the main separator plate (A) and two dowel pins on the torque converter housing. Then install the ATF pump drive gear (B), driven gear (C), and ATF pump driven gear shaft (D). Install the ATF pump driven gear with its grooved and chamfered side facing down. Install the main valve body. |