Install and tighten the nut. Remove the 6.0 mm (0.24 in.) pin that was installed to hold the shift lever. Move the shift lever to each position, and verify that the A/T gear position indicator follows the transmission range switch. Allow the front wheels to rotate freely. Start the engine, and check the shift lever operation in all gears. Push the shift lock release, and verify that the shift lever releases. Reinstall the center console. |