NOTE: Put on gloves to protect your hands. Wear eye protection while cutting the glass adhesive with piano wire. Cover interior surfaces to avoid damaging them. Use glass adhesive set P/N 08C73-X0230N. Remove these items: Windshield wiper arms Cowl covers Rearview mirror Front pillar trim, both sides Roof molding Rain sensor, for some models Remove the molding (A) from the upper edge of the windshield (B). If necessary, cut the molding with a utility knife. If the old windshield will be reinstalled, make alignment marks across the glass and body with a grease pencil. Pull down the front portion of the headliner. Take care not to bend the headliner excessively, or you may crease or break it. Apply protective tape along the edge of the dashboard and body. Using an awl, make a hole through the rubber dam and adhesive from inside the vehicle at the corner portion of the windshield. Push a piece of piano wire through the hole, and wrap each end around a piece of wood. |