Check for continuity between ECM/PCM connector terminal A7 and body ground. Is there continuity?
YES | - | Repair short in the wire between the ECM/PCM (A7) and the CKP sensor, then go to Step 18 .
NO | - | Go to Step 25 .
Turn the ignition switch OFF. Replace the CKP sensor, then go to Step 18 . Reconnect all connectors. Turn the ignition switch ON (II). Reset the ECM/PCM with the HDS. Clear the CKP pattern with the HDS. Do the ECM/PCM idle learn procedure. Do the CKP pattern learn procedure. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P0335 is indicated, check for poor connections or loose terminals at the CKP sensor and the ECM/PCM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Troubleshooting is complete.■
Update the ECM/PCM if it does not have the latest software, or substitute a known-good ECM/PCM. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P0335 is indicated, check for poor connections or loose terminals at the CKP sensor and the ECM/PCM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | If the ECM/PCM was updated, troubleshooting is complete. If the ECM/PCM was substituted, replace the original ECM/PCM.■